{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Chart1","CLAP"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Chart1","index":0,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904"}

{"sheet":"CLAP","index":1,"n_rows":20,"n_cols":55,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["Aerosol sampling efficiency calculator"]
["Global constants",null,null,null,null,null,null,null,null,null,null,{"$f":"3*0.0254","v":7.619999999999999E-2}]
["Temp_air",293.14999999999998,"Kelvin ","Air temperature",null,null,null,null,null,null,null,{"$f":"4*0.0254","v":0.1016}]
["Pres_air",101.3,"kPa","Air pressure"]
["Den_air",{"$f":"1.293*(273.15/Temp_air)*(Pres_air/101.3)","v":1.2047857752004092}," kg/m^3","Air density"]
["Vis_air",{"$f":"0.00001708*((Temp_air/273.15)^1.5)*((393.396)/(Temp_air+120.246))","v":1.8071099473721673E-5}," Pa*s","Air viscosity"]
["Den_particle",1000," kg/m^3","Particle density"]
[null,null,null,null,null,null,null,null,"vertical=90"]
[null,null,null,"m","lpm","m3/s","m/s",null,"degrees","m","degrees","m","U/U0","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um","D_um"]
["Loss","Segment","ID","Diameter","LPM","Flowrate","Velocity","Re_flow","Incline","Length","BendAngle","BendRadius","VelRatio",10,1E-3,{"$f":"O10*10^0.1","v":1.2589254117941673E-3},1.5848931924611136E-3,1.9952623149688798E-3,2.5118864315095803E-3,3.1622776601683798E-3,3.9810717055349734E-3,5.0118723362727246E-3,6.3095734448019355E-3,7.943282347242819E-3,1.0000000000000005E-2,1.258925411794168E-2,1.5848931924611145E-2,1.9952623149688809E-2,2.5118864315095819E-2,3.1622776601683819E-2,3.9810717055349762E-2,5.0118723362727276E-2,6.3095734448019386E-2,7.9432823472428235E-2,0.10000000000000012,0.12589254117941687,0.15848931924611154,0.1995262314968882,0.25118864315095835,0.31622776601683839,0.39810717055349787,0.50118723362727313,0.63095734448019436,0.79432823472428293,1.0000000000000018,1.2589254117941695,1.5848931924611165,1.9952623149688835,2.511886431509585,3.1622776601683857,3.9810717055349807,5.0118723362727335,6.3095734448019467,7.9432823472428336,10.000000000000023]
[]
[]
["Total","Inlet",1,{"$f":"12/64*2.54/100","v":4.7625000000000002E-3},1,{"$f":"E13/60000","v":1.6666666666666667E-5},{"$f":"flowvelocity($F13,$D13)","v":0.93559715147377165},{"$f":"retube($D13,$G13,Temp_air,Pres_air)","v":297.06339101080744},0,{"$f":"3*2.54/100","v":7.6200000000000004E-2},null,null,null,{"$f":"efficiencysettling(N$10,Temp_air,Pres_air,Den_particle,$D13,$J13,$I13,$G13)*efficiencydiffusion(N$10,Temp_air,Pres_air,$D13,$J13,$G13)*EfficiencyInertiaTurbulent(N$10,Temp_air,Pres_air,Den_particle,$D13,$J13,$G13)","v":0.93547646102199167},0.64132201978203451,0.72346513379539323,0.78692126722817501,0.83594234915179821,0.87402457802058531,0.90372126257005181,0.92685659072285986,0.94478278311460906,0.95855994275613698,0.96905293892781286,0.97697598876835856,0.98291402215424672,0.98733761249071861,0.99061788022317265,0.99304223408209036,0.99482990786461234,0.99614614849219563,0.99711438438521149,0.99782618213677399,0.99834911336939947,0.99873280477490645,0.99901348385419453,0.99921731049677065,0.9993627348452303,0.99946206400851023,0.99952235985604798,0.9995457212171257,0.99952891139351774,0.99946215969879504,0.99932678450494095,0.99909104694273176,0.99870331156965619,0.99808106991629142,0.99709354659464711,0.99553431624752198,0.99307841793491236,0.98921556800630117,0.98314689691221802,0.97362690531406149,0.95872525677493514,0.93547646102199145]
["Bend","Bend",2,{"$f":"12/64*2.54/100","v":4.7625000000000002E-3},1,1.6666666666666667E-5,0.93559715147377165,297.06339101080744,null,null,90,{"$f":"20/64*2.54/100","v":7.9375000000000001E-3},null,{"$f":"EfficiencyInertiaBend(N$10,Temp_air,Pres_air,Den_particle,$D14,$K14,$L14,$G14)","v":0.92385724817203996},1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0.99770776712383891,0.99351496907135828,0.98670293941284726,0.97546274750029827,0.95653246142526138,0.92385724817203907]
["Total","Channel",3,6.205251901167083E-3,1,1.6666666666666667E-5,0.55111221333553839,227.99467648088253,90,{"$f":"24/64*2.54/100","v":9.5250000000000005E-3},null,null,null,0.99999139845133445,0.89055329860535182,0.91667024702491917,0.93696687320858119,0.95262755411132305,0.96460377736727287,0.97367963368852462,0.98050130030126481,0.98559358620264303,0.98937441127346082,0.99217018224710096,0.99423159278672524,0.99574860359786932,0.99686366802044546,0.99768279160573459,0.99828442028120024,0.99872638157944438,0.99905119523229202,0.99929007730487784,0.99946592831672476,0.99959554699758002,0.99969126169826739,0.99976212750808624,0.99981480105148468,0.99985417691673872,0.99988384892149784,0.99990644455720834,0.99992387005389793,0.99993749442134561,0.99994829200348168,0.99995695454729017,0.99996397729818731,0.99996972121150318,0.99997445475130586,0.99997838079825541,0.99998165404682382,0.99998439217444535,0.99998668166664806,0.99998857664414886,0.99999008454702687,0.99999112202809259,0.99999139845133445]
["Bend","Bend",4,6.205251901167083E-3,1,1.6666666666666667E-5,0.55111221333553839,227.99467648088253,null,null,90,{"$f":"8/64*2.54/100","v":3.1749999999999999E-3},null,0.97462546288770435,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0.99874853512287298,0.99547515424313771,0.99061513358429398,0.98369599632046512,0.97462546288770358]
["Total","Tube",5,{"$f":"12/64*2.54/100","v":4.7625000000000002E-3},1,1.6666666666666667E-5,0.93559715147377165,297.06339101080744,0,{"$f":"1*2.54/100","v":2.5399999999999999E-2},null,null,null,0.97807230293636882,0.80752735403703146,0.85196606642359973,0.88655519469841271,0.91353348201567741,0.93451504419532394,0.95072275335775935,0.96313353707554816,0.97255094084835758,0.97963778476969099,0.9849336111700937,0.98886918341918462,0.99178174761057547,0.99393084755455696,0.99551346881015013,0.99667751762084222,0.99753316082381405,0.99816197938016316,0.9986241386047785,0.99896388386673241,0.99921368557631407,0.99939732588848651,0.99953217016078177,0.99963081452724645,0.99970225444123384,0.99975268003181528,0.99978597122556678,0.99980393407748824,0.99980628245525105,0.99979031921217698,0.99975020474459464,0.99967561619653511,0.99954948541820876,0.9993443252046994,0.99901636305634534,0.99849624358246902,0.99767435236901114,0.99637772035706584,0.99433378781963488,0.99111375879190855,0.98604448152024626,0.97807230293636871]
["Total to filter",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRODUCT(N13:N17)","v":0.82383969376691901},{"$f":"PRODUCT(O13:O17)","v":0.46120426070006321},{"$f":"PRODUCT(P13:P17)","v":0.56500597236543371},0.65367413075371494,0.72748482018987981,0.78787786772183921,0.83657421446806357,0.87528043734789185,0.90561206016322593,0.92906366970119603,0.94697961899278948,0.96052858167077182,0.97069177158651754,0.97826748532663688,0.9838882728278463,0.98804488596512596,0.99111191434663326,0.99337180031778061,0.99503559300269762,0.99625995977993831,0.99716062926752014,0.99782273313191505,0.99830858888387275,0.99866342830561583,0.99891949226454879,0.99909881719700921,0.99921494256738563,0.99927366392102712,0.99927282107663162,0.99920092233621827,0.99903415168703913,0.99873097970460878,0.99822315526191641,0.99740117380316751,0.9960912333830334,0.99401903856928753,0.98848236619303842,0.97800198568368668,0.96020175602067648,0.93245399187759448,0.88950304003760838,0.82383969376691735]
["ChannelArea",{"$f":"16/64*0.0254*12/64*0.0254","v":3.0241874999999994E-5}]
["ChannelDia",{"$f":"SQRT(4*B19/PI())","v":6.205251901167083E-3}]